@name 
@inputs P:wirelink 
@outputs W A S D ACT SHIFT SPACE CONTROL M1
@persist 
@trigger 

W=P["W",number]
A=P["A",number]
S=P["S",number]
D=P["D",number]
ACT=P["Active",number]
SHIFT=P["Shift",number]
SPACE=P["Space",number]
CONTROL=P["Control",number]
M1=P["Mouse1",number]

