N@Remote Probe Controller
I@Left Right Forward Back Reload Space Alt Shift Turn Vert Active Sync AYaw APitch P0 PP
O@Mul XL XR YL YR ZR ZL Hovcon Hover Pitch Yaw Radio Use Fire Grab Strength Z
XL=XR=YL=YR=0
Mul=(Shift*100)+(1*!Shift)
GPitch=recv(Sync,4), GYaw=recv(Sync,5), Groll=recv(Sync,6)
A=Active -> B=(Shift*100)+(1*!Shift);

RollFlat=Groll < 60 | Groll > -60
RollUp=Groll > 60 | Groll < -60 

XL=(-Forward+Back)+A*-(Turn)
XR=(-Forward+Back)+A*(Turn)

RollFlat==1 -> YL=(Right-Left), ZL=0;
RollFlat==1 -> YR=(Right-Left), ZR=0;
RollUp==1 -> ZL=(Right-Left),YL=0;
RollUp==1 -> ZR=(Right-Left), YR=0;

Hover = (B/(20*Shift +1*!Shift))*(Vert)
Z+=20
Pitch = !Alt*GPitch - Alt*APitch
Yaw = !Alt*GYaw + Alt* AYaw
Use=Reload
Hov=Hovcon
Hovcon==1 & Space==1 & ~Space==1-> Hov=0;
Hovcon==0 & Space==1 & ~Space==1 -> Hov=1;
Hovcon=Hov
X=recv(Sync,1),Y=recv(Sync,2),Z=recv(Sync,3)+20
Radio=send(X,Y,Z)
Fire=P0*A,Grab=PP*A,Strength=10000
